**Solar Hot Water Collector**



Frame from cedar 2x4s to reduce weight



Use lightweight corregated roofing for energy absorber



Double layer insulation Reflectix & board insulation



Board insulation on bottom of panel



Use copper tubing painted black as energy transfer mode



Cover panel in 6 mil poly



Double hot water solar collector on tracker system